# Roads stakeout reports

To display the Confirm staked deltas screen before you store a point, select the View before storage check box in the Stakeout options screen and then select the required format in the Stakeout deltas format field.

If you chose to install a Language and Help Files language pack when you installed the Trimble Access software, stakeout report formats are installed to the controller in the language of your choice. If you did not choose to install a language pack you can install it at any time by running Trimble Installation Manager. See Installing Trimble Access

The following stakeout report formats are installed with Trimble AccessRoads:

- Road – Catch + offsets

  Provides details of all the standard road staked deltas plus a list of the horizontal and vertical distances to each of the cross‑section positions from the staked offset position. The reported horizontal and vertical distances include the applied horizontal and vertical construction offsets.

- Road – Stake markup

  Provides a simplified stakeout display that presents the vertical distance (cut/fill) to the road design position. Appropriate station and offset values and cross‑section details (in the case of catch point staking) are reported, based on the road stakeout method.

- Road – XS details

  Provides all the standard road staked deltas details as well as a list of the cross‑section elements (left and right) that define the design cross‑section at the selected station.

Stylesheets for additional roading reports can be downloaded from the Software and utilities page of the Trimble Access Help Portal.