# To stake an offset point

When staking a point using the default GNSS stake method To the point you can stake an offset point defined by an azimuth and offset from the point.

You can also define a second offset point on the same azimuth as the first offset point.

1. When navigating to the point, tap Offset.

2. Use the fields in the Offset screen to configure staking out points (1) at an azimuth (2) from a point (3) and offset by a horizontal distance (4).

   The elevation for each offset point can be defined by:

   - Slope from point – the elevation is computed by a slope from the elevation of the point selected to stake.
   - Delta from point – the elevation is computed by a delta from the elevation of the point selected to stake.
   - Key in – the elevation is keyed in.

   If the point has no elevation, the elevation for the offset points must be keyed in.

3. Tap Accept.

   The map shows the selected point and the first offset point.

4. Navigate to the offset point. See Stakeout navigation.

5. When the point is within tolerance, measure the point. Tap Store.

   If you have defined a second point, it is shown on the map.

6. Navigate to the second offset point.

7. When the point is within tolerance, measure the point. Tap Store.

   If you are staking points from a list, the software returns to the stakeout point list.