# To end the survey

When you have measured or staked out all points required, do the following:

1. Tap and select Measure or Stakeout and then tap End GNSS survey.

2. If the survey was an RTK Internet survey then the software may ask whether to disconnect the internet connection:

   - Tap Yes to end the connection to the modem, which also ends the corrections stream.

   - Tap No to end the corrections stream but leave the receiver online ready for the next survey.

   To avoid unintentional use of cellular data and VRS hours, the software always ends the corrections stream when the survey ends, regardless of whether the message is shown or not shown, or whether you select Yes or No in response to the message.

3. When prompted to power down the receiver, tap Yes.
4. Turn off the controller before disconnecting the equipment.
5. If you set up your own base station for the survey:
   1. Return to the base station.
   2. If required, reconnect the controller to the base receiver.
   3. Tap and select Measure or Stakeout and then tap End GNSS base survey.
   4. If the controller was logging base data, in the Base screen tap End.