# Receiver settings

To view the configuration of the connected GNSS receiver, tap and hold on the receiver icon in the status bar.

The Receiver settings screen shows information about the type, firmware version, and capabilities of the connected receiver.

Receiver capabilities

Receiver capabilities shown in the Receiver settings screen may include the following:

#### Tracking

The Tracking group shows information about the GNSS satellite constellations that can be tracked using the connected GNSS receiver.

#### RTK

The RTK group shows the RTK capabilities of the connected GNSS receiver, including:

- Broadcast message formats supported by the receiver (for example, CMR+ and CMRx).

- Support for Trimble IonoGuard™ technology for ionospheric disturbance mitigation.

#### RTCM

The RTCM group shows the RTCM broadcast message formats supported by the connected GNSS receiver.

#### RTX

The RTX group shows RTX subscription information, including the subscription expiry date, for the connected GNSS receiver.

#### OmniSTAR

The OmniSTAR group shows OmniSTAR subscription information, including the subscription expiry date, for the connected GNSS receiver.

#### Trimble GNSS Subscriptions

The Trimble GNSS Subscriptions group shows information for the GNSS receiver subscription, including the subscription expiry date.

This group is shown only for receivers that have configurable options provided by subscription, for example when connected to an R780 or R750 receiver.

Receiver configuration softkeys

Use the softkeys at the bottom of the screen to configure additional settings.

To configure:

- GNSS eBubble options, tap eBubble. See GNSS eBubble tilt sensor.
- the RTX satellites that are being used, tap RTX SV. See To view RTX status.
- Wi‑Fi settings for the receiver, tap Wi‑Fi. See Receiver Wi-Fi settings.
- a Bluetooth connection to the receiver, tap Bluetooth. See Bluetooth connections.