# Set out position requirements

Set out positions typically define bolt hole or drill hole locations within the tunnel, and are also used to define blast holes in the tunnel face or holes for installing pipes. All set out positions are defined by station and offset values and a method.

You can key in set out positions as part of the tunnel definition using the Set out screen in Trimble Access. Alternatively, you can design the set out positions in Trimble Business Center and then save them as a TXL file for use in Trimble Access, or you can import set out positions from a CSV file. To key in or import set out positions, see To add set out positions.

Setting out positions using Trimble Access Tunnels refers to the process of staking out the designed positions, and physically marking the location of set out points on the tunnel surface so that drilling equipment can be guided to the correct location of each point for drilling the hole and installing the bolt or pipe. See To set out predefined positions.

Set out position methods

Supported types of set out positions are:

- End-face blast holes
- Bolt holes using the following methods:
  - Radial
  - Horizontal
  - Vertical
  - Multiple radial
- Pipes

Refer to the following diagram:

1

Blast hole

2

Radial

3

Horizontal

4

Vertical

5

Multiple radial

6

Alignment

7

Offset center

8

Interval

9

Pipes

Blast hole set out

Refer to the diagram below to set out positions for blast holes.

1

Blast hole position

2

Design position

3

Design surface

4

Tunnel surface

5

Tunnel alignment

Bolt hole set out

Refer to the diagram below to set out positions for bolt holes defined by the radial (including multiple radial), horizontal, and vertical methods.

1

Set out position defined radial

2

Set out position defined horizontal

3

Set out position defined vertical

4

Design position

5

Design surface

6

Tunnel surface

7

Center for radial position

Pipe set out

Set out pipe positions to install an arch of pipes that extend lengthwise along the planned tunnel alignment to reinforce the roof of the working area. Typically, a series of regularly spaced and overlapping arches of pipes (a pipe umbrella or canopy tube) are installed throughout the sequential excavation of the tunnel.

1

Alignment

2

Pipe umbrella

3

Horizontal offset (pipe start)

4

Vertical offset (pipe start)

5

Horizontal offset (pipe end)

6

Vertical offset (pipe end)

7

2D distance along the alignment.

Imported set out position requirements

You cannot import Multiple radial set out points.

The required format for the CSV file is:

StartStation, EndStation, Type, HorzOffset, VertOffset, Code, Direction, Surface, ExtraHorzOffset, ExtraVertOffset, Length.

See the following examples for the format for each set out method:

Set out positions | Method | Values | Example
--- | --- | --- | ---
End face blast holes | Blasthole | StartStation, EndStation, Type, HorzOffset, VertOffset, Code | 40,60,Blasthole,0.5,‑0.5,Blast hole
Radial bolt holes | Radial | StartStation, EndStation, Type, HorzOffset, VertOffset, Code, Direction, Surface, HorzCenter, VertCenter | 0,40,Radial,‑3.2,2.2,Bolt hole,,S2,1.05,0.275
Horizontal bolt holes | Horizontal | StartStation, EndStation, Type, HorzOffset, VertOffset, Code, Direction, Surface | 0,20,Horizontal,,3.1,Bolt hole,Right,S2
Vertical bolt holes | Vertical | StartStation, EndStation, Type, HorzOffset, VertOffset, Code, Direction, Surface | 0,,Vertical,3.2,,Bolt hole,Up,S2
Pipes | Pipe | StartStation, EndStation, Type, HorzOffset, VertOffset, Code, EndHorzOffset, EndVertOffset, PipeLength | 0,,Pipe,‑1.0,2.5,Pipe,-1.1,2.6,5.0

- The Surface name, Code, Horizontal offset, and Vertical offset values are optional.
- If no Surface name is specified, or the Surface name is not applicable for the specified station range, the first template surface suitable for the station range is used.
- The Method value must be one of the following: Blasthole, Horizontal, Vertical, Radial, Pipe.
- The Direction value must be one of the following: Up, Down, Left, Right, or empty (for a radial offset, blast hole, or pipe).