# To add template positions

After adding templates, you must specify the station at which the Tunnels software starts to apply each template. For more information on how the software does this, see Template application.

1. Select Template positioning.
2. To specify a new position at which template(s) should be applied:
   1. Tap Add.
   2. Enter the Start station.
   3. In the Template field, select the template to use. To create a gap in the tunnel definition, select None.
   4. Select the surface from the selected template you want to use.
   5. Tap Store.
3. Continue adding positions where templates should be applied, as required.
4. Tap Options to specify if the templates are applied Vertical or Perpendicular to the vertical alignment.

5. When you are done, tap Close.

6. Tap Accept.

7. Enter the other tunnel components, or tap Store to store the tunnel definition.