# Stakeout navigation deltas

The navigation information displayed during stakeout is user-definable and different configurations can be set up for the following item types:

- Points

- Points on a line, arc, polyline, or road

- Line, arc, polyline, or road

- Surface

## To edit the stakeout deltas

1. Tap and select Settings / Survey styles / <Style name> / Stakeout to configure the survey style to display the stakeout deltas as you usually use them.

   To change the deltas during stakeout, tap Options in the stakeout screen or tap and hold in the navigation pane.

2. In the Deltas group, tap Edit.

   1. In the Deltas list, tap a delta to change whether the delta is displayed. A check mark indicates the delta will be shown. When fewer deltas are shown they are displayed in a larger font.

   2. To reorder the deltas, tap and hold a delta and drag it up or down the list.

   3. Tap Accept.

3. If you are using a controller with a smaller screen, or you want to fit more navigation deltas on the screen, set the Show stakeout graphics switch to No.

4. To save the changes you have made to the stakeout deltas to the current survey style, tap Save to style.

5. Tap Accept to return to the Stakeout screen.

Available deltas

Available deltas for different items are listed below. However, if a specific delta is not applicable to the selected method used to stake out the item then the delta is either not shown or shows null.

Deltas: Points

Available deltas for points are:

- Go North/South

- Go East/West

- Go Left/Right

- Go Forward/Backward

- Go In/Out (conventional surveys only)

- Delta H.Ang (conventional surveys only)

- Go Left/Right (angle) (conventional surveys only)

- H.Ang reqd. (conventional surveys only)

- Elevation

- V.Dist

- Design elevation

- Azimuth

- H.Dist

- Northing

- Easting

- DTM elevation

- V. Dist surface

- Perp. Dist to surface

- Code

Deltas: Points on a line, arc, polyline, alignment or road

Available deltas for points on a line, arc, polyline, alignment or road are the same as for a line, arc, polyline, or road, with the addition of:

- Go Forward/Backward Relative to line

- Go Left/Right Relative to line

- Grade to line

- Distance along line

- H. Dist to end

- Side slope (Design)

- Side slope (Calculated)

- Fill slope (as staked)

- H.Dist to hinge point

- V.Dist to hinge point

- S.Dist to hinge

- Station: Reference string

- H.Offset: Reference string

- V.Dist cross slope (roads only)

- Code

- Horizontal const. offset (when staking construction offsets)

- Vertical const. offset (when staking construction offsets)

- Station const. offset (when staking construction offsets)

- Design station

- Design string

- Design horizontal offset

- Design vertical offset (not available for roads)

- Design slope (alignments or roads only)

- Slope (roads only)

- Surface slope (alignments or roads only)

- Distance along line is the 3D or slope distance from the start of the line (or arc, polyline, or road) to the current location. H.Dist to end is the 2D or horizontal distance from the current location projected to the end of the line (or arc, polyline, or road).

- Design slope displays the slope of the template element that precedes the string you have selected to stake when you are staking To a string, Station on a string or To the nearest string. When staking by Side slope from alignment it displays the slope of the side slope directly below your current position. Slope displays the slope of the template element directly below your current position. Surface slope displays the slope of the surface at right angles to the horizontal alignment and directly below your current position.

Deltas: Line, arc, polyline, alignment or road

Available deltas for a line, arc, polyline, alignment or road are the same as for points, with the addition of:

- Go Left/Right Relative to line

- Grade to line

- Distance along line

- H. Dist to end

- Station

- H.Offset

- Grade to line

- Station: Reference string

- H.Offset: Reference string

- V.Dist cross slope (roads only)

- Code

- Horizontal const. offset (when staking construction offsets)

- Vertical const. offset (when staking construction offsets)

- Station const. offset (when staking construction offsets)

- Design station

- Design string

- Design horizontal offset

- Design vertical offset (not available for roads)

- Design slope (alignments or roads only)

- Slope (roads only)

- Surface slope (alignments or roads only)

- Distance along line is the 3D or slope distance from the start of the line (or arc, polyline, or road) to the current location. H.Dist to end is the 2D or horizontal distance from the current location projected to the end of the line (or arc, polyline, or road).

- Design slope displays the slope of the side slope directly below your current position, unless you are staking To a string, Station on a string or To the nearest string when it displays the slope of the template element that precedes the string you have selected to stake. Surface slope displays the slope of the surface at right angles to the horizontal alignment and directly below your current position.

Deltas: Surface

Available deltas for surfaces are:

- Northing

- Easting

- Elevation

- Design elevation

- V.Dist

- Perp. Dist

- Code