# Status bar

The status bar appears at the top of the screen when a job is open. It provides information about the equipment that is connected to the controller and access to commonly used functions.

Conventional survey status bar

GNSS survey status bar

Common status bar items

Items that usually appear on the status bar are:

Item | Name | Description
--- | --- | ---
| Menu button | Tap to view the menu.
| Application icon | Shows the current Trimble Access app. If you have only one app installed, the status bar always shows the General Survey icon. To change to a different app, tap the icon and then select the app to switch to. In portrait mode, the app icon does not appear on the status bar. To change to a different app, tap and select the name of the current app (for example, General Survey) and then in the Choose application screen, tap the name of the app to switch to.
| Date and time | Shows the current date and time.
| Status line | The status line displays a message when an event or action occurs. Tap the status line to switch from one instrument to another during an integrated survey. The status line appears at the far right of the status bar. In portrait mode it appears below the status bar.

Battery status

The Battery status area on the status bar shows the status of the battery in the controller and devices connected to the controller. If the controller has more than one battery, the power level of each battery is shown.

To view the Battery status screen, tap the battery status area of the status bar.

Conventional survey status

During a conventional survey, values for the current horizontal angle or vertical angle and distance are shown in the status line.

Instrument status

To view the:

- Instrument functions screen, tap the Instrument icon in the status bar.
- Instrument settings screen, tap and hold the Instrument icon in the status bar.

The Instrument icon indicates the type of connected instrument. Symbols are added to the Instrument icon to indicate status.

Icon | Indicates
--- | ---
| The software is connected to a Trimble SX10 or SX12 scanning total station. The instrument height is shown when a station setup is complete.
| The SX10/SX12 is connected to the controller using Wi‑Fi. The Wi‑Fi signal strength is indicated below the Wi‑Fi icon.
| The SX10/SX12 EDM is in standard (STD) mode. It averages the angles while a standard distance measurement is taken.
| The SX10/SX12 EDM is in standard (STD) mode. The laser pointer is enabled (SX12 only).
| The SX10/SX12 EDM is in standard (STD) mode. The instrument is locked onto the target (prism).
| The SX10/SX12 EDM is in Tracking (TRK) mode. It constantly measures distances and updates in the status line.
| The SX10/SX12 EDM is in Tracking (TRK) mode and DR mode is enabled.
| The SX10/SX12 EDM is in Tracking (TRK) mode. DR mode is enabled. The laser pointer is enabled (SX12 only).
| The white circle over the instrument indicates target illumination (TIL) is enabled.
| The software is connected to a Trimble VX spatial station or Trimble S Series total station. The instrument height is shown when a station setup is complete.
| The software is connected to a Trimble C5 total station.
| The software is connected to a Trimble M3 total station.
| The software is connected to a Spectra Geospatial FOCUS 50 total station.
| The software is connected to a Spectra Geospatial FOCUS 30 or 35 total station.
| The instrument is locked onto the target (prism).
| The instrument is locked and measuring to the target (prism).
| The instrument is in Fast Standard (FSTD) mode. It averages the angles while a fast standard measurement is taken.
| The instrument is in Standard (STD) mode. It averages the angles while a standard distance measurement is taken.
| The instrument is in Tracking (TRK) mode. It constantly measures distances and updates in the status line.
| The instrument is locked to the target (prism) and receiving an EDM signal back from the prism.
| The laser pointer is on (DR mode only).
| The high power laser pointer is on.
| Radio signals from the robotic instrument are no longer being received.
| The compensator is disabled.
| Auto‑connect is disabled. Tap the icon once to restart auto‑connect. Tap the icon again to configure Auto‑connect settings.

Target status

To change the target or target settings, tap the Target status icon in the status bar. See Target height.

Icon | Indicates
--- | ---
| The prism is locked. "1" indicates that target 1 is in use. The prism constant (in millimeters) and target height are shown to the right of the icon. When measuring a point with a dual-prism offset, two prism constants are shown.
| The instrument is in Direct Reflex mode.
| The rotating target icon with a pulsing red halo indicates that the instrument has Autolock enabled but is not currently locked onto a target.
| FineLock is enabled.
| Long Range FineLock is enabled.
| GPS Search is enabled.
| Interrupted Target Measurement is enabled.

GNSS survey status

During a GNSS survey, precision information for the current position is shown in the status line.

Satellites

The number below the satellite icon indicates the number of satellites in the solution if you have started a survey, or the number of satellites being tracked if you have not yet started a survey. To view the Satellites screen, tap .

If [A] or [B] appears next to the number of satellites in an RTK survey, then an independent subset of satellites is being used. See To use independent subsets of satellites tracked in RTK surveys.

GNSS receiver

To view the:

- GNSS functions screen, tap the GNSS receiver icon in the status bar.
- Receiver settings screen, tap and hold the GNSS receiver icon in the status bar.

The GNSS receiver icon indicates the type of connected GNSS receiver:

Icon | Indicates
--- | ---
| Trimble R780 receiver, where IMU tilt compensation is enabled and the IMU is aligned. Measurements are corrected for receiver tilt. Precision values for the current pole tip position are displayed.
| Trimble R780 receiver, where IMU tilt compensation is enabled but the IMU is not aligned. Measurements are not corrected for receiver tilt. No precision values are displayed.
| Trimble R780 receiver, where IMU tilt compensation is not enabled. The receiver is operating in GNSS-only mode. Precision values for the APC are displayed.
| Trimble R12i receiver, where IMU tilt compensation is enabled and the IMU is aligned. Measurements are corrected for receiver tilt. Precision values for the current pole tip position are displayed.
| Trimble R12i receiver, where IMU tilt compensation is enabled but the IMU is not aligned. Measurements are not corrected for receiver tilt. No precision values are displayed.
| Trimble R12i receiver, where IMU tilt compensation is not enabled. The receiver is operating in GNSS-only mode. Precision values for the APC are displayed.
| Trimble R12 receiver
| Trimble R10 receiver
| Trimble R8s receiver
| Trimble R8 receiver
| Trimble R580 receiver
| Trimble R2 receiver
| Trimble DA2 receiver
| Trimble R750 receiver
| Trimble R9s or NetR9 Geospatial receiver
| Trimble R7 receiver
| Trimble SPS986 GNSS Smart Antenna, where IMU tilt compensation is enabled and the IMU is aligned. Measurements are corrected for receiver tilt. Precision values for the current pole tip position are displayed.
| Trimble SPS986 GNSS Smart Antenna, where IMU tilt compensation is enabled but the IMU is not aligned. Measurements are not corrected for receiver tilt. No precision values are displayed.
| Trimble SPS986 GNSS Smart Antenna, where IMU tilt compensation is not enabled. The receiver is operating in GNSS-only mode. Precision values for the APC are displayed.
| Trimble TDC650 handheld GNSS receiver
| Spectra Geospatial SP60 receiver
| Spectra Geospatial SP80 receiver
| Spectra Geospatial SP85 receiver
| Spectra Geospatial SP90m receiver
| Auto‑connect is disabled. Tap the icon once to restart auto‑connect. Tap the icon again to configure Auto‑connect settings.

Real-time correction information

To view more detailed status information, tap the real-time correction information area of the status bar.

Icon | What it shows
--- | ---
| Radio signals are being received.
| Radio signals are no longer being received.
| Cellular modem signals are being received.
| Cellular modem has hung up, or has stopped receiving corrections.
| Radio signals are being received. xFill® is ready to provide RTK if required.
| Radio signals are no longer being received. xFill is enabling RTK to continue.
| SBAS or OmniSTAR® signals are being received.
| RTX satellite signals are being received and an RTX position is being generated.
| Data is being received from the RTX satellite but an RTX position cannot be generated yet.
| An RTX survey is running but data is not being received from the RTX satellite.
| A point is being measured.
| Continuous points are being measured.
| A point is being measured using a Trimble receiver with IMU tilt compensation.
| Continuous points are being measured using a Trimble receiver with IMU tilt compensation.
| A GNSS RTK survey is running and base data from a GNSS internet source is being streamed to the rover.
| A GNSS RTK survey is running and base data streaming from a GNSS internet source is paused. Base data streaming automatically restarts when required.
| A GNSS RTK survey is running and base data from a GNSS internet source is being received but the solution from the receiver is not yet using that base data.
| A GNSS RTK survey is running and base data streaming from a GNSS internet source is stopped. The base station connection to the GNSS internet source is maintained, but the real‑time base data will not be streamed to the rover.
| A GNSS RTK survey is running but base data from a GNSS internet source cannot be received.

Antenna details

The current antenna height is shown below the antenna icon. If the antenna icon is the same as the receiver icon then the internal antenna is being used.

To change the current antenna settings, tap the antenna icon in the status bar.