# Storing the current receiver position

If the controller is connected to a GNSS receiver, or you are using a controller with internal GPS, you can quickly store the current position of the receiver without having to start a survey. This is especially useful for storing waypoints so that you can easily return to locations of interest.

When using a controller with internal GPS, a connected GNSS receiver is always used in preference to the internal GPS.

1. To store the current position:
   - Tap the receiver icon in the status bar and select Position. To store the position, tap Store. See Current position information.
   - When navigating to a location, in the Navigate to point screen tap Position.
   - Make sure no features are selected in the map and then tap and hold an empty space in the map and select Store a point.
2. Make sure the value in the Antenna height field is correct.
3. Tap Store.