# To capture a snapshot on measure

1. Connect to the instrument.

2. To view the Video feed from the instrument, tap in the map toolbar or tap the Instrument icon in the status bar to open the Instrument functions screen and then tap Video.

3. Tap and then tap Settings:
   1. Make sure that Snapshot on measure is enabled. See Snapshot options.
   2. To draw the instrument crosshairs on the image or to add an information panel to the image, select the Annotate snapshot check box and then configure the annotation options. See Annotate snapshot options.
   3. Set the other options as required and then tap Accept.

4. In the video screen, aim to the target and then tap Measure.

   If no feature code is set then the captured snapshot is assigned to the measured point.

5. If a feature code is required, select it in the Code field.

6. If the feature code has a file name attribute, tap Attrib.

   The name of the captured image appears in the file name field.

   If there are multiple File name attribute fields, the file name appears in the first file name field.

   If there are multiple codes entered for the point, an attribute form appears for each code with attributes. The file name is entered into the first file attribute field that appears.

7. Tap Store.