# To export LandXML string roads from Trimble Novapoint

For best results when using LandXML string roads in the Trimble Access Roads software, export files using Trimble Novapoint version 21.00 or later.

1. Start Trimble Novapoint and select a project.
2. From the Output ribbon, select Export to file.
3. Select the features to export.
4. Select LandXML as the output format.
5. To export the road as a centerline with associated:
   - break lines, select InfraBIM Breaklines as the conversion rule (or your own modified conversion file).
   - irregular lines, select Irregular lines as the conversion rule (or your own modified conversion file).
6. Select Finish to export the file.

It is also possible to export LandXML files from Trimble Novapoint version 16.00 through 20.00. For more information, refer to the Trimble Novapoint User Guide.