# To configure the conventional survey style

1. Tap and select Settings/ Survey styles.

2. Do one of the following:

   - Tap <Style name> and then tap Edit.
   - Tap New. Enter a name for the style and then tap Accept.

3. Select each of the options in turn, and set them to suit your equipment and survey preferences.

   To... | See...
   --- | ---
   configure settings for the instrument | Instrument configuration
   set parameters for topo points | Conventional point options
   configure the software to warn when duplicate points are measured | Duplicate point tolerance options
   configure stakeout settings | Stakeout options
   use a laser rangefinder | Laser rangefinders
   use an echo sounder | Echo sounders
   use a utility locator | Utility locators

4. Tap Store.