# Conventional point options

As part of configuring the survey style for a conventional survey, you can configure the settings for topo points measured during the survey.

To configure these settings, tap and select Settings / Survey styles / <style name> / Topo point.

In the Measure display field, select how the observations are displayed on the controller. For a list of the available options and the corrections that are applied, see Instrument corrections.

In the Auto point step size field, set the increment size for automatic point numbering. The default is 1, but you can use larger step sizes and negative steps.

Select the View before storage check box to view observations before they are stored.