# Subdivide a line

1. To open the Subdivide a line form, you can:

   - In the map, select the line to be subdivided. Tap and hold in the map and select Subdivide a line.

   - Tap and select Cogo / Subdivide a line. Enter the name of the line.

     If the line does not already exist, tap and select Two points. Enter the start point and end point to define the line.

2. To set the code of the created points, tap Options and select the name or code of the line that is to be subdivided in the Subdivide points code field.

3. Subdivide the line using one of the following methods:

   For the Fixed segment length method:
   1. In the Method field, select Fixed segment length.

   2. Enter the segment length (2), and any horizontal offset (3) and vertical offset from the line.

   3. Enter the Start at station(4), the End at station(5), and the Start point name.

   4. Tap Start. The software calculates the new points (4, 6, 7, or 8, 9, 10).

      The names of the created points are incremented from the Start point name and are stored in the job.

   For the Fixed number of segments method:
   1. In the Method field, select Fixed number of segments.

   2. Enter the number of segments, and any horizontal offset (2) and vertical offset from the line.

   3. Enter the names of the Start at station(3), the End at station(4), and the Start point name.

   4. Tap Start. The software calculates the new points (3, 5, 4, or 6, 7, 8).

      The names of the created points are incremented from the Start point name and are stored in the job.