# To report the definition of an RXL road

To generate an HTM text report of the defined RXL road:

1. Select the road. In the map, tap the road to select it.

   To select the road from the list:

   1. Tap and select Define.
   2. Tap RXL road.
   3. Select the road.
2. Tap Edit.
3. Tap Report.
4. To include only a part of the road definition in the report, select a different Start station and End station.

5. Tap Accept.

   The report appears in your browser. It shows the offset, coordinates, elevation, and code for each position in the cross section for the selected stations. The values reported are for the resolved cross sections, that is, they include any superelevation and widening values that may have been applied, and any interpolation between different templates.

   If the definition includes additional points these are included in the report in a separate section after the Road Cross-Section Points.