# Offsetting a line or polyline

1. In the map, select the line/polyline to offset.
2. Tap and hold in the map and select Offset line/Offset polyline.
3. Enter the Horizontal offset and/or Vertical offset value. To change the offset direction, tap next to the appropriate offset field.
4. To change how distances are calculated, tap Options. See Cogo settings.
5. Enter the name and, if required, the code for the new line/polyline.
6. If you are offsetting a polyline, enter the Start station and Station interval.
7. Tap Store.